### Carrier Text Display The information below provides a FULL description of this microblock and all of its properties. What information you see and what you can do with it depends on your license and the application you are in, and in some cases, a controller's driver version.
Microblock family | Carrier microblocks
Icon and symbol |
What it does | This microblock lets you display text for a CCN point on a Properties page or Graphics page. NOTE To display on a Graphics page, add a Single-line Text control to the graphic in ViewBuilder. In the Control Properties window, type ccn_disp_text in the Property field.
#### Properties
Display Name | The microblock label used in the interface. You can use any characters (including spaces) in this field, except for the " character.
Reference Name RefName | Use the default reference name unless you want a more descriptive name for graphics or network links. Limitations: lower case only limited to 40 characters cannot begin with a number must be unique within a control program
Path | Use the information below to format a valid path for the microblock you are using to read or write to the CCN point. Each item in the path is limited to 8 alpha-numeric characters. Check Editable if you want the path to be editable in the WebCTRL® interface. Path format: CCN://LINK/<table name>/<point name><:instance#><@force level> LINK represents the CCN device defined in the CCN Controller microblock. <table name> - Use one of the following: Definition table name:Data table name Example: `CCN://LINK/MYTABLE:MYDATA1` Definition table name:Instance number Example: `CCN://LINK/MYTABLE:1` Data table name Example: `CCN://LINK/MYDATA1` Where: Definition table name is the name of the POC table that describes the data structure of the child tables. Data table name is the name of the table instance that contains the variable or field being referenced. Instance# is the table instance number <point name> Example: `CCN://LINK/.../HEATSP` `` <:instance#> (Optional) - Use the instance number of the point name if the table has more than one point with the same name. <@force level> (Optional) - The force level being written to (a value 1–15) Example: `CCN://LINK/HOLIDAYS:HOLIDAY1/HEATSP@4` You can edit the address/path of a CCN point in one of the following places in the WebCTRL® interface: The Details tab of a Point Properties dialog box The Address column on the Properties > Network Points page
Communications Enabled | Check to enable network communications for this microblock. Uncheck when troubleshooting.
Editing Privilege | Preset - Each microblock property has an appropriate privilege or role assigned to it. You can use Global Modify in the WebCTRL® interface to find out what the actual privilege is. CAUTION If you change the Editing Privilege from Preset, the privilege you select will be used for all properties of this microblock, which is not always desirable.
Show Property Page Text | Check to show this microblock's value on the equipment's Properties page.