### Properties pages Properties pages are automatically generated from control programs created in the EIKON® application. Use Properties pages to: View the status of a piece of equipment. See Colors and status in the WebCTRL® interface. View or change the equipment or microblock properties currently stored in the controller Commission equipment
Click for details below To view or edit properties Point types
#### To view or edit properties Select a piece of equipment or a microblock on the Geographic or Network tree, then click Properties. NOTE You must resolve any condition described in red text at the top of the page before a Properties page can obtain current information from its controller. To change a property: Click Accept. NOTES Right-click a value, then select Details to view and change properties in the microblock pop-up. Right-click a value, then select Global Modify to view and change the property in other control programs. A yellow dashed box around a value indicates the value is locked.
#### Point types A point name on the Properties page is followed by a code that tells you the point type. The table below describes each code.
Code | Point type
--- | ---
AI | Analog Input
ANI | Analog Network Input
ANI2 | Analog Network Input 2
ANO | Analog Network Output
ANO2 | Analog Network Output 2
AO | Analog Output
ASVI | BACnet Analog Sensed Value Input
AV | Analog Value
BAI | BACnet Analog Input
BALM | BACnet Alarm
BAO | BACnet Analog Output
BAV | BACnet Analog Value
BBI | BACnet Binary Input
BBO | BACnet Binary Output
BBV | BACnet Binary Value
BFM | Floating Motor
BI | Binary Input
BLSTAT | LogiStat Zone Sensor with Optional OAT Display
BMSV | BACnet Multi-State Value
BNI | Binary Network Input
BNI2 | Binary Network Input 2
BNO | Binary Network Output
BNO2 | Binary Network Output 2
BO | Binary Output
BPTA | Pulse to Analog Input
BPWM | Pulse-Width Output
BRS | RS Sensor
BRSF | RS Sensor Fan
BSVI | BACnet Binary Sensed Value Input
BTLO | Timed Local Override
BTRN | Trend Log
BV | Binary Value
DI | Digital Input
DO | Digital Output
EVT | BACnet Alarm
LAN AI | LAN Analog Input
LAN AO | LAN Analog Output
LAN DI | LAN Digital Input
LAN DO | LAN Digital Output
LSTAT | LogiStat Zone Sensor
POLLAVG | Average Analog Properties
POLLMAX | Maximum Analog Properties
POLLMIN | Minimum Analog Properties
POLLTOT | Total Analog Properties
PTA | Pulse to Analog Input
TLO | Timed Local Override