# What's new in v7.0
Click for details below What's new in the WebCTRL® application What's new in the ViewBuilder application What's new in the SiteBuilder application What's new in the EIKON® application
## What's new in the WebCTRL® application
Feature | Improvement
--- | ---
Custom reports | Custom reports are now created and managed through the new Report Manager. You can export one or more custom reports to a file so that they can be imported into another system. A custom report can provide data for the following new items on a Graphics page: Data table Chart Color map See What's new in the ViewBuilder application for more information on the above items. NOTE To support upgraded systems, you can still create and access legacy (v6.5 and earlier) custom reports.
Scheduled Reports | You can set up a report to run on a recurring basis. The report is saved as a file (PDF, CSV, or XLS), and you can choose to have it automatically emailed to someone.
Default Email Server Configuration settings | The Email Server Configuration settings, used by scheduled reports and the Send Email alarm action, are now located on the System Settings > General tab.
Send Email alarm action | This alarm action can use the default Email Server Configuration settings defined in System Settings, or you can enter settings specific to the alarm action.
New FDD alarm categories | The WebCTRL® application now has two new alarm categories, FDD Comfort and FDD Energy.
Send Web Service Request alarm action | This new alarm action sends a web service request to a third-party server when an alarm occurs.
Disabling the Schedules feature | You can disable the Schedules feature in System Settings so that Schedules are no longer visible in the WebCTRL® interface for systems that do not use them.
Improved Foreign Device Registration | If your system requires that WebCTRL® be registered as a foreign device to a BBMD, you can now define a second BBMD in case the first one fails.
System Statistics | The System Statistics button on the General tab of System Settings now includes the following totals: Number of controllers Number of controllers that can run control programs Number of points, regardless of vendor
Re-authentication of operator for 21 CFR Part 11 | If an operator is required to record a reason for making system changes, the operator is now required to re-enter their system password in the box where they record the changes.
Run External Program alarm action | This alarm action can now be set up only when running WebCTRL® Design Server.
Add-ons | By default, the WebCTRL® application now allows only signed add-ons that are supported by Automated Logic®. This default can be overridden in SiteBuilder. See What's new in the SiteBuilder application. NOTE Some previously installed add-ons may not run after upgrade. See the "After the upgrade" in the WebCTRL® v7.0 Upgrade Guide for conditions and solutions.
Security enhancements | Apache Tomcat web server has been upgraded to v7.0.82. The WebCTRL® application has been upgraded to Java 8 update 144.
64-bit server | The WebCTRL® v7.0 application will run only on a server with a 64-bit operating system. If you have a previous WebCTRL® version that is running on a 32-bit server, you will need to upgrade your server before installing v7.0.
2 new optional packages | The WebCTRL® Superset package allows the discovery of and communication with Carrier Open and CCN controllers. The Multi-CCN package allows for multiple CCN Bus 0's for a WebCTRL® system that has the WebCTRL® Superset optional package. See the CCN Integration Guide for information on using this feature.
WAP device support | This has been removed from the WebCTRL® application. Smart phone support introduced in v6.5 replaced this functionality.
## What's new in the ViewBuilder application
Feature | Improvement
--- | ---
Data tables and charts | These new controls on a Graphics page pull data from a WebCTRL® report. The chart control allows you to specify a line chart, pie chart, horizontal bar chart, or vertical bar chart. Data table Vertical bar chart
Color maps | A Graphics page color map shows specified colors for various conditions that are defined in a WebCTRL® report.
Default graphic size | The default graphic size in ViewBuilder is now 1666 x 849 pixels.
Local Variables | ViewBuilder now preserves local variables through cut/copy and paste, as well as when importing a .viewsymbol.
Layers | ViewBuilder now preserves layers when importing a .viewsymbol. If cutting/copying a selection assigned to layers, you must hold Shift while pasting in a new file to preserve layer assignments.
Downloading a Custom Equipment Touch file | If a .touch file contains many screens or large images that cause the file to become too large for the controller's memory, you can download only the name of the .touch file to the controller instead of the entire file. You will then need to manually copy the .touch file to your device.
## What's new in the SiteBuilder application
Feature | Improvement
--- | ---
Improved security settings | To increase security, the WebCTRL® application defaults to the following settings: If your system is set to use TLS, the WebCTRL® application automatically uses TLS 1.2. The WebCTRL® application requires SOAP applications to run over HTTPS. The WebCTRL® application allows only add-ons that have been approved by Automated Logic®. NOTE If needed, you can override these defaults in SiteBuilder; however, doing so will lessen the security of your system.
## What's new in the EIKON® application
Feature | Improvement
--- | ---
Support for the following new optional features has been added to EIKON®. When released, you can download them from https://accounts.automatedlogic.com/dowload under Software Products and Updates > v7.0 installs and updates.
Improved Edit Order | Provides more flexibility and reduces the time needed to create property pages for equipment.
Translation Assistance Tool | Simplifies the process of creating non-English control programs.