### Binary Status The information below provides a FULL description of this microblock and all of its properties. What information you see and what you can do with it depends on your license and the application you are in, and in some cases, a controller's driver version.
Microblock family | Sys Out microblocks
Icon and symbol |
What it does | This microblock displays a yes/no, on/off, open/closed, or true/false value from the control program on the Properties page. You can use this microblock to display the value of another microblock that would not normally appear on the Properties page.
#### Properties TIPS Alt+click any value in the WebCTRL® or Field Assistant interface to view property details, including its editing privilege and expression (location path) for use on graphics. You can right-click some properties in the EIKON® Property Editor and select Make editable or Make read-only to determine that property's functionality in your system.
Reference Name RefName | Use the default reference name unless you want a more descriptive name for graphics or network links. Limitations: lower case only limited to 40 characters cannot begin with a number must be unique within a control program
Type | Select Text Defined Below to use the values in the Active Text and Inactive Text fields. Or select the Inactive and Active text you wish to use from the Type droplist.
Inactive Text | The Inactive Text your system displays when the microblock's output is off, or false.
Active Text | The Active Text your system displays when the microblock's output is on, or true.
Property Page Text
Show Property Page Text | Check to show this microblock's value on the equipment's Properties page.
Property Page Text | You can edit the microblock description that appears on the Properties page. See "Editing Properties page text using special characters" and "Formatting a microblock property" in EIKON® Help.