### Set Color If True The information below provides a FULL description of this microblock and all of its properties. What information you see and what you can do with it depends on your license and the application you are in, and in some cases, a controller's driver version.
Microblock family | Control microblocks
Icon and symbol |
What it does | This microblock broadcasts the selected color for the control program when it is activated. The microblock's input accepts an on or off signal. When the input is on, the selected color is broadcast. If the input is off, the microblock does not generate any color. This allows you to use more than one Set Color If True microblock in a control program, as long as only one of these microblocks is activated at a time.
#### Properties TIPS Alt+click any value in the WebCTRL® or Field Assistant interface to view property details, including its editing privilege and expression (location path) for use on graphics. You can right-click some properties in the EIKON® Property Editor and select Make editable or Make read-only to determine that property's functionality in your system.
Reference Name RefName | Use the default reference name unless you want a more descriptive name for graphics or network links. Limitations: lower case only limited to 40 characters cannot begin with a number must be unique within a control program
Editing Privilege | Preset - Each microblock property has an appropriate privilege or role assigned to it. You can use Global Modify in the WebCTRL® interface to find out what the actual privilege is. CAUTION If you change the Editing Privilege from Preset, the privilege you select will be used for all properties of this microblock, which is not always desirable.
Color | Select the color that is to be displayed with the input is on.