### Low Peak Recorder The information below provides a FULL description of this microblock and all of its properties. What information you see and what you can do with it depends on your license and the application you are in, and in some cases, a controller's driver version.
Microblock family | Log microblocks
Icon and symbol |
What it does | This microblock records the lowest and previous lowest value of a microblock in a control program. You determine when the values are recorded and when the lowest value is transferred to the previous lowest value. For example, if you want to record the lowest outside air temperature for each day, this microblock can record today's lowest temperature and yesterday's lowest temperature. The microblock's analog input receives the value that is to be recorded. When the rec input is on, the microblock monitors the input value and transfers the lowest value received to the microblock's primary output. This output value is transferred to the prev output when the rset input is turned on.
#### Properties TIPS Alt+click any value in the WebCTRL® or Field Assistant interface to view property details, including its editing privilege and expression (location path) for use on graphics. You can right-click some properties in the EIKON® Property Editor and select Make editable or Make read-only to determine that property's functionality in your system.
Reference Name RefName | Use the default reference name unless you want a more descriptive name for graphics or network links. Limitations: lower case only limited to 40 characters cannot begin with a number must be unique within a control program
Property Page Text
Show Property Page Text | Check to show this microblock's value on the equipment's Properties page.
Property Page Text | You can edit the microblock description that appears on the Properties page. See "Editing Properties page text using special characters" and "Formatting a microblock property" in EIKON® Help.