### Graphics pages You can view and adjust your system from Graphics pages, which include navigation maps, floor plans, and equipment. Some typical items that may appear on a graphics page are: Button or switch to turn equipment on or off Input field to set a property value Drop-down list to select a state Interactive zone sensor to override an unoccupied schedule Setpoint graph to adjust setpoints Trend graph to view trend information Link to jump to another WebCTRL® page or to the Internet A data table, chart, or color map that pulls information from a custom report. NOTES Right-click a value, then select Details to view and change properties in the microblock pop-up. Right-click a value, then select Global Modify to view and change the property in other control programs. A yellow dashed box around a value indicates the value is locked. If a graphic does not fit in the action pane, right-click it and select Scale to Fit to make it fit the action pane. Select Scale to Fit again to return the graphic to its original size. When a chart that is based on a report is displayed on a Graphics page, you can hover over various points on the chart to see values. You can also click on each item in the legend to turn that information on and off. See Using a custom report as the source for a Graphics page for more information on a chart.
Click for details below To attach a graphic in the WebCTRL® interface To edit a graphic on a WebCTRL® client To organize multiple graphics for a tree item To control equipment using an interactive zone sensor
3. #### To attach a graphic in the WebCTRL® interface On the navigation tree, right-click the item that you want to attach a graphic to, then select Configure. Equipment graphic only: If the system has other control programs of this type, select which control programs you want to change. NOTES If the control program is in an IP router, the second option will change the graphic for all control programs of this type only on the IP network. If the control program is on the network below an IP router, the second option will not change the graphic for the router's control programs of this type. Do one of the following:
   If the graphic is... |
   --- | ---
   In the Views Available list | a. Select the graphic, then click Attach. b. Click Accept.
   Not in the Views Available list | a. Click Add New. b. Browse to select the view file. c. Click Open. d. Click Continue. e. Click Close. f. Click Close again.
NOTES Select a graphic in the Attached list to edit the following information for the graphic: Display Name–The name that appears in the Graphics button drop-down list Category–The name of the category that multiple graphics may be sorted into in the Graphics button drop-down list NOTE Changes to Display Name or Category apply only in the WebCTRL® interface and are not retained if you export source files. Reference Name–The name that is used to create links to the graphic in ViewBuilder Default View–Sets the selected graphic as the default view if the tree item has multiple graphics. The default graphic is bolded in the Attached list. NOTE The default graphic is initially set in SiteBuilder. Included in download–Equipment graphics only. Select to have the .view file included in an All Content download so that it can be uploaded by Field Assistant. The graphic will have beside it in the Attached list. Requires 4.x or later drivers. You can click Delete Unused at the bottom of the Views section to delete all unattached graphic files from your system.
#### To edit a graphic on a WebCTRL® client On a WebCTRL® client, you can get a copy of a graphic from the server, edit it, then put it back on the server. To get the graphic On the WebCTRL® Geographic tree, right-click the item that the graphic is attached to, then select Configure. At the bottom of the Views section, click Edit Existing. Select the graphic you want to edit. Click Save Browse to the folder you want to put the file in. Click Save. Click Close. Click Close again. To put the edited graphic back on the server On the WebCTRL® Geographic tree, right-click the item that the graphic is attached to, then select Configure. At the bottom of the Views section, click Add New. Browse to select the .view file. Click Open. Click Continue. Click Close. Click Close again.
#### To organize multiple graphics for a tree item In the WebCTRL® interface, you can create categories and assign graphics to them so that the Graphics button drop-down menu has the graphics arranged by category. This is typically done in ViewBuilder or SiteBuilder. See "To define WebCTRL® navigation" in ViewBuilder Help and "To attach graphic files" in SiteBuilder Help. To add a Graphics category in the WebCTRL® interface On the System Configuration tree, click to the left of the Categories folder, then select Graphic. Click Add. Type the Category Name and Reference Name. Optional: Select a privilege so that only operators with that privilege can access graphics in the category. Click Accept. NOTES To edit a category, select the category, make your changes, then click Accept. To delete a category, select the category, click Delete, then click Accept. To assign a graphic to a category in the WebCTRL® interface On the Geographic tree, right-click the item that the graphic is attached to, then select Configure. Under Views, select the graphic in the Attached list. Select the category in the Category field. Click Accept.
#### To control equipment using an interactive zone sensor An equipment graphic may include an interactive zone sensor that provides you with the following control.
If the sensor is a... | You can...
--- | ---
ZS | Click to raise the setpoint or to lower the setpoint. Click to override the schedule and put the zone in an occupied state. To cancel an override, continue clicking until the display shows 0. See that the zone is in an occupied state when the green LED is lit.
RS Standard, Plus, or Pro | Click the WARMER or COOLER button to adjust the setpoint. Click the MANUAL button to override the schedule and put the zone in an occupied state. Click the INFO button to cycle through the following information: Outside air temperature, if enabled in the control program Override time remaining Heating setpoint Cooling setpoint See the Occupied/Unoccupied state in the display.
RS Pro-F | Click the WARMER or COOLER button to adjust the setpoint. Click the MANUAL button to override the schedule and put the zone in an occupied state. Click the INFO button to cycle through information such as: Outside air temperature Override time remaining Heating setpoint Cooling setpoint Click the FAN button to adjust the fan speed. Click the MODE button to perform customer-specific functions. See the Occupied/Unoccupied state in the display.
LogiStat | Click to raise the setpoint or to lower the setpoint. Click to override the schedule and put the zone in an occupied state. See that the zone is in an occupied state when the red LED is lit.