## Retired microblocks The microblocks listed in the left column below have been retired from the EIKON® microblock menu. However, they are still supported by the EIKON® application, controllers, and the WebCTRL® application. If you open a control program that contains one of these microblocks, you can edit properties in the microblock and copy and paste it to other applications if necessary. For applications to be used in v5.5 or later WebCTRL® systems, use the microblocks in the right column below. These microblocks have configurable options that provide the functionality of the retired microblocks.
Instead of this retired microblock... | Use...
| BACnet Multi-State Value Parameter - 20 states | BACnet Multi-State Value Parameter
| BACnet Multi-State Value Status - 20 states | BACnet Multi-State Value Status
| Zone Setpoint | BACnet Setpoint
| Zone Setpoint with Demand | BACnet Setpoint
| Zone Setpoint - Plus | BACnet Setpoint
| Zone Setpoint with Learning Adaptive Optimal Start | BACnet Setpoint
| Zone Setpoint with Demand and Learning Adaptive Optimal Start | BACnet Setpoint
| Zone Setpoint - Plus with Learning Adaptive Optimal Start | BACnet Setpoint
| BACnet Time Clock | BACnet Time Clock with TLO and Override Status
| BACnet Time Clock with TLO | BACnet Time Clock with TLO and Override Status
To add retired microblocks to a control program If needed, you can add any of the retired microblocks to a control program. Select Tools > Configure Tools. Click Add. Select add-retired-microblocks.logic-plugin, then click Open. Click OK. Select Tools > Add Retired Microblocks. Select the microblock you want. Click Add. Click in the workspace to place the microblock.